Skip to Tutorial Content

## Introduction

Welcome to the tutorial on Reliability Testing! In this tutorial, you will learn about different types of reliability tests and how to apply them. These models are commonly applied in industries like aerospace, automotive, and electronics, where improving product reliability over time is critical.

## What is Reliability Testing?

Reliability testing is a process to ensure that a product or system performs its intended functions under specified conditions over a defined period. For example, in the automotive industry, we may want to design a car that runs without breaking down for 5 to 10 years.

## Why is Reliability Testing important?

Reliability testing helps organizations predict the future reliability of products, reduce failure rates, and lower costs associated with repairs and downtime.

## Learning Objectives

By the end of this tutorial, you will be able to:

1. Define key reliability growth concepts, including Crow-AMSAA and Duane models.
2. Fit a reliability growth model to real-world data using R.
3. Interpret reliability growth plots and identify trends.
4. Apply the Crow-AMSAA model to assess reliability growth.
5. Explain fundamental concepts of accelerated life testing, including the use of Arrhenius and Power Law Models.
6. Conduct an accelerated life test with real-world datasets, utilizing R for analysis.
7. Analyze plots that illustrate the relationships in accelerated life testing, identifying key patterns and data trends.
8. Utilize Arrhenius and Power Law models to evaluate the impact of stress factors on product reliability.

## Reliability Growth Analysis

Reliability Growth Analysis (RGA) is a method to monitor and improve, or grow, the reliability of a product or system over time. Often the product is improved due to changes in the design throughout the testing period.

## The Duane Model

The Duane Model was developed by J. T. Duane in 1964 and provides a simple and graphical way to observe and analyze whether failure rates are improving as changes are made to a product or system.

Specifically, the Duane Model is a log-log plot of the cumulative Mean Time Between Failures (MTBF) vs cumulative time.

The slope of the line on the plot indicates the rate of reliability growth:

- A positive slope means that the system is improving (reliability is growing, the failure rate is decreasing).
- A zero slope means there is no change in reliability (the system is stable).
- A negative slope indicates that reliability is worsening (the failure rate is increasing).

### The Duane Model: Reliability Growth vs Deteriation

Take the following example Duane Plot. Adjust the Beta value input to see the failure rate both decreasing and increasing.

### Beta Value:

### The Duane Model Equation

The cumulative MTBF at any time \(t\) can be expressed as:

\[ CMBTF(t) = K \cdot t^{\beta - 1} \]

Where:

- \(CMBTF(t)\) is the cumulative MTBF at time \(t\),

- \(K\) is a constant related to the initial failure rate,

- \(t\) is the cumulative operating time,

- \(\beta\) is the reliability growth parameter (slope of the line on the log-log plot).

  - If \(\beta > 1\), the system reliability is improving (the failure rate decreases over time).
  - If \(\beta = 1\), the system reliability is constant (no improvement or degradation).
  - If \(\beta < 1\), the system reliability is deteriorating (the failure rate increases over time).

### Exercises

## ReliaGrowR

### Getting Started with ReliaGrowR

For this tutorial, we will use ReliaGrowR: a R package for Reliability Growth Analysis.

First, check if ReliaGrowR is installed in R and install if not.

    if(!(require(ReliaGrowR))){install.packages('ReliaGrowR')}

Next, set up some cumulative time and failure data. Then use the `duane_plot` function to fit a Duane Model to the data.

    times <- c(100, 200, 300, 400, 500)
    failures <- c(1, 2, 1, 3, 2)
    fit <- duane_plot(times, failures, line_col = "red")

### Exercises

## The Crow-AMSAA Model

The Crow-AMSAA or Non-Homogeneous Poisson Process (NHPP) model was developed by Larry H. Crow and is based on the Army Materiel Systems Analysis Activity (AMSAA) testing framework.

Specifically, the Crow-AMSAA Model is a plot of the cumulative number of failures vs cumulative time.

Similar to the Duane Model, the shape of the model indicates the rate of reliability growth:

- A model fit with downward curvature means that the system is improving (reliability is growing, the failure rate is decreasing).
- A linear model means there is no change in reliability (the system is stable).
- A model fit with upward curvature indicates that reliability is worsening (the failure rate is increasing).

### The Crow-AMSAA Model: Reliability Growth vs Deteriation

Take the following example Crow-AMSAA model. Adjust the Beta value input to see the failure rate both decreasing and increasing.

### Beta Value:

### The Crow-AMSAA Model Equation:

The cumulative number of failures up to time \(t\) is given by:

\[N(t) = \lambda_0 \cdot t^{\beta}\]

Where:

- \(N(t)\) is the cumulative number of failures,

- \(\lambda_0\) is the scale parameter.

- The Shape Parameter (\(\beta\)) indicates whether the system is improving or deteriorating:

  - If \(\beta\) > 1, failures are increasing over time, indicating that reliability is worsening.
  - If \(\beta\) < 1, failures are decreasing, indicating that reliability is improving over time.
  - \(\beta\) = 1 implies a constant failure rate (no growth or degradation).

### Crow-AMSAA with ReliaGrowR

To run a Crow-AMSAA model with ReliaGrowR, first set up some cumulative time and failure data:

    times <- c(100, 200, 300, 400, 500)
    failures <- c(1, 2, 1, 3, 2)

Then use the `rga` function to fit the model and the `plot_rga` function to plot the results:

    result <- rga(times, failures)
    plot_rga(result, line_col = "orange")

### Exercises

### The Piecewise Weibull NHPP Model

The Piecewise Weibull NHPP model is an extension of the standard NHPP model that includes different segments or phases of time that follow separate Weibull failure distributions. This model is particularly useful when a system experiences changes in failure behavior over different development phases, such as the initial, interim and final phases of a development process.

### The Weibull Distribution

The Weibull intensity function for each time segment \(i\) is modeled as:

\[\lambda_i(t) = \frac{\beta_i}{\eta_i} \left( \frac{t - t_{i-1}}{\eta_i} \right)^{\beta_i - 1}\]

Where:

- \(\lambda_i(t)\) is the failure intensity in time interval \(i\),
- \(\beta_i\) is the shape parameter for interval \(i\),
- \(\eta_i\) is the scale parameter (characteristic life) for interval \(i\),
- \(t_{i-1}\) is the start time of the interval.

### Example

To run a Piecewise Weibull NHPP with ReliaGrowR, first, set up some cumulative time and failure data and specify a breakpoint:

    times <- c(100, 200, 300, 400, 500, 600, 700, 800, 900, 1000)
    failures <- c(1, 2, 1, 1, 1, 2, 3, 1, 2, 4)
    breakpoints <- 400

Then run the rga and plot the results:

    result <- rga(times, failures, model_type = "Piecewise Weibull NHPP", breakpoints = breakpoints)
    plot_rga(result)

### The Piecewise Weibull NHPP with Change Point Detection

The Piecewise Weibull NHPP with Change Point Detection is an advanced model to identify changes in failure behavior and model system reliability. This method builds on the Piecewise Weibull NHPP model by introducing the concept of change points, which represent the time when the underlying failure behavior changes. Detection of change points involves statistical techniques that analyze failure data to automatically identify when the behavior changes, allowing for a more precise segmentation of the model into different Weibull distributions.

### Example

To run a Piecewise Weibull NHPP with Change Point Detection with ReliaGrowR, first, set up some cumulative time and failure data:

    times <- c(100, 200, 300, 400, 500, 600, 700, 800, 900, 1000)
    failures <- c(1, 2, 1, 1, 1, 2, 3, 1, 2, 4)

Then run the rga and plot the results:

    result <- rga(times, failures, model_type = "Piecewise Weibull NHPP")
    plot_rga(result)

## Accelerated Life Testing

Accelerated Life Testing (ALT) is a method to estimate the life of a product or system under normal operating conditions by subjecting it to accelerated stress levels in a controlled environment. The goal is to identify potential failure modes and predict how long the product will last under normal conditions without having to wait for failures to occur naturally over a longer time period.

### Accelerated Life Testing: Stress vs Life

Take a product that is designed to last 10,000 hours. Waiting for it to fail naturally could take months. With ALT, you might increase the operating temperature of the product, causing it to fail faster.

The following plot shows the relationship between the acceleration or stress factor and the expected life of the product: as the acceleration factor increases, the expected life tends to decrease. Adjust the acceleration factor input to see this impact in action.

### Acceleration Factor:

## The Arrhenius Model

The Arrhenius Model is widely used in ALT to model the effect of temperature on the rate of chemical reactions, which directly relates to the degradation or failure rate of materials.

The Arrhenius equation is expressed as:

\[k(T) = A \cdot e^{-\frac{E_a}{k_B \cdot T}}\]

Where:

- \(k(T)\) is the reaction rate at temperature \(T\)
- \(A\) is the pre-exponential factor
- \(E_a\) is the activation energy
- \(k_B\) is the Boltzmann constant
- \(T\) is the absolute temperature in Kelvin

### The Arrhenius Life Model

The Arrhenius model relates the life of a product to temperature using the following form:

\[\log(\text{Life}) = -\frac{E_a}{k_B} \cdot \frac{1}{T} + \log(A)\]

Where \(\log(\text{Life})\) is the natural logarithm of the expected life.

By fitting this model to test data, you can estimate the activation energy and predict product life under normal operating conditions.

## WeibullR.ALT

For this tutorial, we will use WeibullR.ALT, an extension of the WeibullR package for Accelerated Life Testing.

First, check if WeibullR.ALT is installed in R and install if not.

    if(!(require(WeibullR.ALT))){install.packages('WeibullR.ALT')}

For this example, we will use the data set `MeekerData` that comes prepackaged with `WeibullR.ALT`. First, load the data set and view the first few samples.

    data <- MeekerData("table10")
    head(data)

The data set contains columns for the time to failure time, event type event (1 = failure, 0 = suspension), quantity of samples qty and temperature as the acceleration factor TempC. Testing was conducted at 4 different temperature levels, 10, 40, 60, and 80 degrees C.

Next, use the `alt.data` function to create a separate object for the data at each temperature level.

    data10C <- alt.data(data[which(data$TempC==10), 1:3],
                        stress = data[which(data$TempC==10), 4][1])
    data40C <- alt.data(data[which(data$TempC==40), 1:3],
                        stress = data[which(data$TempC==40), 4][1])
    data60C <- alt.data(data[which(data$TempC==60), 1:3],
                        stress = data[which(data$TempC==60), 4][1])
    data80C <- alt.data(data[which(data$TempC==80), 1:3],
                        stress = data[which(data$TempC==80), 4][1])

Finally, use the `alt.make` function to fit an Arrhenius-Weibull model to the data.

    arrobj <- alt.make(list(data10C, data40C, data60C, data80C), dist = "weibull",
                    alt.model = "arrhenius", method.fit = "mle")

### Exercises

## The Power Law Model

The Power Law Model is another commonly used model in ALT, particularly for mechanical systems and components. This model describes how a product’s life is affected by a certain stress factor (such as temperature, voltage, or pressure). Unlike the Arrhenius model, which is primarily used for temperature-based stresses, the Power Law Model can be applied to a wide variety of stress factors.

The general form of the Power Law Model is given by:

\[\text{Life}(S) = \frac{A}{S^n}\]

Where:

- \(\text{Life}(S)\) is the expected life under stress level \(S\)
- \(A\) is a constant representing life at a reference stress level
- \(S\) is the applied stress
- \(n\) is the stress exponent that characterizes how sensitive the life is to changes in the stress level

For this example, we will use the data set `NelsonData` that comes prepackaged with `WeibullR.ALT`. First, load the data set and view the class of data.

    data <- NelsonData("table3.1")
    class(data)

    ## [1] "list"

The data is a list of time to failure data at 7 different voltage stress levels, 26KV, 28kV, 30kV, 32kV, 34kV, 36kV, and 38kV.

Next, use the `alt.data` function to create a separate object for the data at each stess level.

    data26 <- alt.data(data$kV26, stress = 26)
    data28 <- alt.data(data$kV28, stress = 28)
    data30 <- alt.data(data$kV30, stress = 30)
    data32 <- alt.data(data$kV32, stress = 32)
    data34 <- alt.data(data$kV34, stress = 34)
    data36 <- alt.data(data$kV36, stress = 36)
    data38 <- alt.data(data$kV38, stress = 38)

Finally, use the `alt.make` function to fit an Power-Weibull model to the data.

    pwrobj <- alt.make(list(data26, data28, data30, data32, data34, data36, data38),
                       dist = "weibull", alt.model = "power")

### Exercises

## Multiple Stress Factors

The Eyring Model is an extension of the Arrhenius model and is commonly used in ALT to account for the combined effects of multiple stressors such as temperature, voltage, and humidity on the failure mechanisms of a product. This model is particularly useful when the product is exposed to environmental factors beyond just temperature.

The general form of the Eyring Model is:

\[\text{Life}(S) = A \cdot \exp\left(\frac{B}{S} + C \cdot S\right)\]

Where:

- \(\text{Life}(S)\) is the expected life under stress level \(S\),
- \(A\) is a constant,
- \(B\) and \(C\) are model parameters,
- \(S\) is the applied stress factor (e.g., temperature, voltage, humidity).

## Parallellization

A common assumption in ALT is that the subset of data at each stress level have the same slope or shape factor. If each model subset has the same slope, then all models appear as parallel plots.

To fit a parallel model to the Meeker data, use the `alt.parallel` function.

    prlobj <- alt.parallel(arrobj)

Similarly, a parallel model can be fitted to the Nelson data.

    expobj <- alt.parallel(pwrobj)

## Relationship Plots

Another way to view the relationship between the stress factor and the life of a product is with a relationship plot. A relationship plot is a log-linear plot with the stress factor on the x-axis and the log of the unreliability (failure probability) on the y-axis.

A linear model is fit to the data, which shows patterns indicating how life changes as stress increases.

- A negative slope (decreasing life with increasing stress) indicates that higher stress leads to shorter life.
- A positive slope (increasing life with increasing stress) is less common but indicates that life improves with higher stress.
- A flat slope indicates that higher stress does not have an impact on life.

To fit a relationship plot to the Meeker data, first fit a linear model to the data and then plot the results.

    lnrobj <- alt.fit(prlobj)
    plot(lnrobj, suppress.dev.new = TRUE)

Similarly, a relationship plot can be fitted to the Nelson data.

    lnrobj2 <- alt.fit(expobj)
    plot(lnrobj2, suppress.dev.new = TRUE)

### Exercises

## Summary

In this tutorial, we’ve introduced the concepts of Reliability Growth Analysis and Accelerated Life Testing. You have learned to calculate and visualize reliability using different types of models.

### More resources

WeibullR.plotly is a package for building interactive Weibull models.

WeibullR.shiny is a web application for life data analysis.

### References

- Abernethy, R.B. (2004). The New Weibull Handbook. Fifth Edition.

- Aden-Buie G, Schloerke B, Allaire J, Rossell Hayes A (2023). learnr: Interactive Tutorials for R. https://rstudio.github.io/learnr/, https://github.com/rstudio/learnr.

- Crow, Larry H. (1975). Reliability Analysis for Complex, Repairable Systems. Army Material Systems Analysis Activity, 40. https://apps.dtic.mil/sti/citations/ADA020296

- Fasola S, Muggeo VMR, Kuchenhoff K. (2018). A heuristic, iterative algorithm for change-point detection in abrupt change models. Computational Statistics, 33, 997-1015.

- Govan P (2024). ReliaGrowR: Reliability Growth Analysis. R package version 0.1, https://cran.r-project.org/package=ReliaGrowR.

- Guo, H., Mettas, A., Sarakakis, G. and Niu, P., (2010). Piecewise NHPP models with maximum likelihood estimation for repairable systems. 2010 Proceedings - Annual Reliability and Maintainability Symposium (RAMS), 1-7. https://doi.org/10.1109/RAMS.2010.5448029.

- Duane J. T. (1964). Learning Curve Approach to Reliability Monitoring. IEEE Transactions on Aerospace, 2, 563-566, https://doi.org/10.1109/TA.1964.4319640.

- Meeker W. Q., Escobar L. A., (1998). Statistical Methods for Reliability Data, Wiley-Interscience, New York.

- Nelson W, (1990). Accelerated Testing, Wiley-Interscience, New York.

- Silkworth, David. (2020). WeibullR: An R Package for Weibull Analysis for Reliability Engineers. 43-53. https://doi.org/10.35566/isdsa2019c3.

- Silkworth D, Symynck J (2022). WeibullR: Weibull Analysis for Reliability Engineering. R package version 1.2.1, https://CRAN.R-project.org/package=WeibullR.

- Silkworth D (2022). WeibullR.ALT: Accelerated Life Testing Using ‘WeibullR’. R package version 0.7.2, https://CRAN.R-project.org/package=WeibullR.ALT.

# Reliability Testing