---
title: "State Space Reconstruction"
author: "Wenbo Lv"
date: |
  | Last update: 2026-02-01
  | Last run: 2026-02-01
output: rmarkdown::html_vignette
vignette: >
  %\VignetteIndexEntry{2. State Space Reconstruction}
  %\VignetteEngine{knitr::rmarkdown}
  %\VignetteEncoding{UTF-8}
---



## Methodological Background

Takens theory proves that for a dynamical system $\phi$, if its trajectory converges to an attractor manifold $M$—a bounded and invariant set of states—then there exists a smooth mapping between the system $\phi$ and its attractor $M$. Consequently, the time series observations of $\phi$ can be used to reconstruct the structure of $M$ through delay embedding.

According to the generalized embedding theorem, for a compact $d$-dimensional manifold $M$ and a set of observation functions $\langle h_1, h_2, \ldots, h_L \rangle$, the mapping $\psi_{\phi,h}(x) = \langle h_1(x), h_2(x), \ldots, h_L(x) \rangle$ is an embedding of $M$ when $L \geq 2d + 1$. Here, *embedding* refers to a one-to-one map that resolves all singularities of the original manifold. The observation functions $h_i$ can take the form of time-lagged values from a single time series, lags from multiple time series, or even completely distinct measurements. The former two are simply special cases of the third.

This embedding framework can be extended to *spatial cross-sectional data*, which lack temporal ordering but are observed over a spatial domain. In this context, the observation functions can be defined using the values of a variable at a focal spatial unit and its surrounding neighbors (known as *spatial lags* in spatial statistics). Specifically, for a spatial unit $s$, the embedding can be written as:

$$
\psi(x, s) = \langle h_s(x), h_{s(1)}(x), \ldots, h_{s(L-1)}(x) \rangle,
$$

where $h_{s(i)}(x)$ denotes the observation function of the $i$-th order spatial lag unit relative to $s$. These spatial lags provide the necessary diversity of observations for effective manifold reconstruction. In practice, if a given spatial lag order involves multiple units, summary statistics such as the mean or directionally-weighted averages can be used as the observation function to maintain a one-to-one embedding.

## Usage examples

### Example of spatial vector data

Load the `spEDM` package and its county-level population density data:


``` r
library(spEDM)

popd_nb = spdep::read.gal(system.file("case/popd_nb.gal",package = "spEDM"))
## Warning in spdep::read.gal(system.file("case/popd_nb.gal", package = "spEDM")):
## neighbour object has 4 sub-graphs
popd = readr::read_csv(system.file("case/popd.csv",package = "spEDM"))
## Rows: 2806 Columns: 7
## ── Column specification ─────────────────────────────────────────────────────────
## Delimiter: ","
## dbl (7): lon, lat, popd, elev, tem, pre, slope
## 
## ℹ Use `spec()` to retrieve the full column specification for this data.
## ℹ Specify the column types or set `show_col_types = FALSE` to quiet this message.
popd_sf = sf::st_as_sf(popd, coords = c("lon","lat"), crs = 4326)
popd_sf
## Simple feature collection with 2806 features and 5 fields
## Geometry type: POINT
## Dimension:     XY
## Bounding box:  xmin: 74.9055 ymin: 18.2698 xmax: 134.269 ymax: 52.9346
## Geodetic CRS:  WGS 84
## # A tibble: 2,806 × 6
##     popd  elev   tem   pre slope          geometry
##  * <dbl> <dbl> <dbl> <dbl> <dbl>       <POINT [°]>
##  1  780.     8  17.4 1528. 0.452 (116.912 30.4879)
##  2  395.    48  17.2 1487. 0.842 (116.755 30.5877)
##  3  261.    49  16.0 1456. 3.56  (116.541 30.7548)
##  4  258.    23  17.4 1555. 0.932  (116.241 30.104)
##  5  211.   101  16.3 1494. 3.34   (116.173 30.495)
##  6  386.    10  16.6 1382. 1.65  (116.935 30.9839)
##  7  350.    23  17.5 1569. 0.346 (116.677 30.2412)
##  8  470.    22  17.1 1493. 1.88  (117.066 30.6514)
##  9 1226.    11  17.4 1526. 0.208 (117.171 30.5558)
## 10  137.   598  13.9 1458. 5.92  (116.208 30.8983)
## # ℹ 2,796 more rows
```

Embedding the variable `popd` from county-level population density:


``` r
v = spEDM::embedded(popd_sf,"popd",E = 10)
v[1:5,c(4,5,10)]
##           [,1]     [,2]      [,3]
## [1,]  962.7204 1664.756 1581.4351
## [2,]  919.6000 2408.766 1494.8241
## [3,] 1435.0165 1958.686  813.9077
## [4,] 1488.2727 2066.748 1216.6986
## [5,] 2326.8429 1290.188 1038.3864
```


``` r
plot3D::scatter3D(v[,4], v[,5], v[,10], colvar = NULL, pch = 19,
                  col = "red", theta = 45, phi = 10, cex = 0.35,
                  bty = "f", clab = NA, tickmarks = FALSE)
```

![**Figure 1**. The reconstructed attractors for the variable `popd`.](../man/figures/ssr/fig1-1.png)

<br>

### Example of spatial raster data

Load the `spEDM` package and its farmland npp data:


``` r
library(spEDM)

npp = terra::rast(system.file("case/npp.tif", package = "spEDM"))
npp
## class       : SpatRaster 
## size        : 404, 483, 5  (nrow, ncol, nlyr)
## resolution  : 10000, 10000  (x, y)
## extent      : -2625763, 2204237, 1877078, 5917078  (xmin, xmax, ymin, ymax)
## coord. ref. : CGCS2000_Albers 
## source      : npp.tif 
## names       :      npp,        pre,      tem,      elev,         hfp 
## min values  :   164.00,   384.3409, -47.8194, -122.2004,  0.03390418 
## max values  : 16606.33, 23878.3555, 263.6938, 5350.4902, 44.90312195
```

Embedding the variable `npp` from farmland npp data:


``` r
r = spEDM::embedded(npp,"npp",E = 5,tau = 20)
r[which(!is.na(r),arr.ind = T)[1:5],1:3]
##          [,1]     [,2]     [,3]
## [1,] 2896.833 2933.926 2898.288
## [2,] 3664.286 3071.789 3003.966
## [3,] 3317.337 3090.832 2973.627
## [4,] 3196.011 3107.388 2942.477
## [5,] 3329.188 3080.360 2892.083
```


``` r
plot3D::scatter3D(r[,1], r[,2], r[,3], colvar = NULL, pch = 19,
                  col = "#e77854", theta = 45, phi = 10, cex = 0.01,
                  bty = "f", clab = NA, tickmarks = FALSE)
```

![**Figure 2**. The reconstructed attractors for the variable `npp`.](../man/figures/ssr/fig2-1.png)
